-ChemE Design Day: Thursday 4/20 @ 3 PM

-Design Day: Monday 4/24 @ 5 PM

-compare free bottles to cost of buying PET filament

- compare buy filament vs regrind

- calculate materials cost

- calculate horsepower of motor

- find a payback period

- rework 25% : 25% regrind pellets + 75% PETG virgin pellets

- 25% rework because that's what the bottle industry is doing

- drag flow rate: our data is only 50-60% of it

- future could consider the conical barrel – something for future groups to consider

- other group requested the granulator via the Green Fund